{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":11,"n_cols":6,"rows_kept":11}
["序号","标的物名称","规格/型号","单位","数量","需要验证项目"]
["1","聚偏氟乙烯滤芯（不锈钢内衬,双层膜）","HPVDF-0.2-30-226/C","支",450,"细菌存活、细菌截留（含重复使用）、化学兼容性（含重复使用）、可提取物与浸出物（含重复使用）、现场试验后验证、滤芯完整性检测合格（含多次灭菌后）"]
["2","聚偏氟乙烯滤芯（不锈钢内衬,双层膜）","HPVDF-0.2-20-226/C","支",70,"细菌存活、细菌截留（含重复使用）、化学兼容性（含重复使用）、可提取物与浸出物（含重复使用）、滤芯完整性检测合格"]
["3","聚偏氟乙烯滤芯（不锈钢内衬,双层膜）","HPVDF-0.2-10-226/C","支",10,"细菌存活、细菌截留、化学兼容性、滤芯完整性检测合格"]
["4","聚四氟乙烯滤芯（不锈钢内衬）","PTFE-0.2-30-226/C","支",2000,"细菌存活、细菌截留（含重复使用）、化学兼容性（含重复使用）、可提取物与浸出物（含重复使用）、现场试验后验证、滤芯完整性检测合格（含多次灭菌后）"]
["5","聚四氟乙烯滤芯（不锈钢内衬）","PTFE-0.2-20-226/C","支",60,"细菌截留（含重复使用）、滤芯完整性检测合格（含多次灭菌后）、最大灭菌次数相关材料、反向灭菌可耐受压力及灭菌次数及灭菌温度等相关数据"]
["6","聚四氟乙烯滤芯（不锈钢内衬）","PTFE-0.2-10-226/C","支",10,"细菌截留（含重复使用）、滤芯完整性检测合格（含多次灭菌后）、最大灭菌次数相关材料、反向灭菌可耐受压力及灭菌次数及灭菌温度等相关数据"]
["7","聚四氟乙烯滤芯（不锈钢内衬）","PTFE-0.2-5-226/C","支",50,"细菌截留（含重复使用）、滤芯完整性检测合格（含多次灭菌后）、最大灭菌次数相关材料、反向灭菌可耐受压力及灭菌次数及灭菌温度等相关数据"]
["8","聚四氟乙烯滤芯","PTFE-0.45-30-226/C","支",50,"可提取物与浸出物等相关数据"]
["9","聚偏氟乙烯滤芯","HPVDF-0.45-30-226/C","支",30,"化学兼容性（含重复使用）、可提取物与浸出物"]
["10","聚偏氟乙烯滤芯","HPVDF-0.45-20-226/C","支",600,"化学兼容性（含重复使用）、可提取物与浸出物"]